* temperature gains from shutter data
	eg. temp-gains.s4a.dat

* getPosition(subarray, row, col) 
	use subarray characteristics to get focal plane position
	Thus, rotation can define global rotation

* read all subscans (check to see if adjacent)
	(allow selecting subscans)


