             *** CRUSH User's Manual Extension for SHARC ***

                              Attila Kovacs
                      <attila[AT]submm.caltech.edu>

                       Last updated: 20 May 2014




Table of Contents
=================

1. Introduction
  1.1 Notes of curiosity	
2. Locating Scans
3. Pointing and Extinction Corrections
4. Glossary of SHARC-specific options




#####################################################################
1. Introduction
#####################################################################


This document contains information specific to using CRUSH-2 to reduce SHARC
data. It is assumed that you are already familiar with the contents of the main
CRUSH-2 README (inside the distribution directory), especially its Section 1
(Getting Started).

If you run into difficulty understanding the concepts in this document, you
will probably find it useful to study the main README document a little longer.



1.1 Notes of curiousity
=======================

SHARC represented a particular challenge for integrating into CRUSH (which is
why it was interesting), since CRUSH was designed for total-power data, whereas
SHARC produces only a dual-beam differential stream via a chop, which requires
the extra step of deconvolution. The deconvolution, and map accumulation, 
happens in Fourier domain, and the dual-beam image that is synchronized to the
time-stream is dynamically generated in each iteration, for each scan. 

The deconvolution method is essentially an Emerson II (Emerson 1995) type 
algorithm with some extra use of well-placed noise weighting. The new SHARC 
module mainly serves as a demo for what CRUSH can do for dual-beam (and 
multibeam) reductions in general. CRUSH can be further tweaked to work with 
arbitrary wobble patterns too, if there is desire to adapt it...



#####################################################################
2. Locating Scans
#####################################################################


SHARC scans were stored in user-specified data files (stored in poorly 
documented VAX-binary format), with each file containing data from multiple 
scans. So, before  accessing any given scan, you must specify the data file via
the 'file' option, or via the combination of 'datapath' and file. E.g., say 
your data file is '/home/sharc/mydata.dat'. Then you can specify this file 
either as:

   crush sharc [...] -file=/home/sharc/mydata.dat [...]

or as:

   crush sharc [...] -datapath=/home/sharc -file=mydata.dat [..]

(Clearly, the second is advantageous when you want to reduce scans from 
multiple files in the same location.)

Next you can obtain a listing of the scans in any given file using the 'list' directive. E.g.

   crush sharc [...] -file=myfile.dat list

will list the scan entries stored in 'myfile.dat'.

Every row of an OTF scan constitutes a separate scan entry in the data file. 
While the scan headers state how many OTF rows each complete scan should have, 
the number of rows recorded in the data may often be fewer (aborted scans or 
crashes) or more (often by +1). Therefore, there is no fool-proof automatic 
detection of which scan rows 'belong' together. Instead you can specify which
entries to treat as belonging to the same 'master' scan. Suppose you judge
that entries 3-12 are part of the same OTF, and 15-19 another, and 22 is a
single pass over the same data. Then you may reduce these together as:

   crush sharc [...] -file=myfile.dat 3-12 15-19 22

I.e., unlike for other instruments, ranges for SHARC specify entries that are
to be treated as one scan (not a range of scans as for other instruments).



#####################################################################
3. Pointing and Extinction Corrections
#####################################################################

This works the same way as for SHARC-2, so you should read the corresponding
section of sharc2/README. But, in short you can 'fazo' and 'fzao' to correct
the pointing, and 'tau.225GHz' to set a 225GHz tau value. E.g.:

   crush sharc [...] -fazo=-49.5 -fzao=10.2 -tau.225GHz=0.043 3-12 [...]

There is one small difference, however, is that the 'sharc' tau relation
includes the bolometer nonlinearity (which for SHARC-2 is treated separately).



#####################################################################
4. Glossary of SHARC-specific options
#####################################################################

   chopper.throw=X	@Advanced
			Overrider. Specify the chopper throw (arcsecs) to use 
			instead of the value recorded in the data file.

   deconvolve.above=X	@Expert
			Set the deconvolution threshold to X. Usually 0<X<2.
			When the transfer function (Fourier transform) of the 
			chop pattern is below this value, the corresponding
			Fourier components are considered no measured (i.e.
			set to zero). 		

   file=<path>		Specify the data file either as a fully specified
			path, or relative to the path set by the 'datapath'
			option.	

   pixelsize=X		@Expert
			Set the SHARC pixel spacing to X arcseconds. By 
			default, the nominal 5" spacing is assumed.

   source.type=multibeam	@Advanced
				Setting the source type to 'multibeam' 
				(default) will produce deconvolved maps. 
				Otherwise, CRUSH will produce dual-beam
				maps.


------------------------------------------------------------------------------
Copyright (C)2014 -- Attila Kovacs <kovacs@astro.umn.edu>
